;/************************************************************
;*     File:   oxpci2.inf
;*            
;*  Description:
;*             Installs the serial ports behind a PCI bridge
;*
;*
;************************************************************/

[Version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%mfg%
;CatalogFile=Oxpci2.cat      ; .cat file (no different binaries)
DriverVer=09/26/2005, 5.1.2

[DestinationDirs]
DefaultDestDir  = 11                ;LDID_SYS

; Install class "Ports"
;----------------------------------------------------------
[ClassInstall]
AddReg=PortsClass.AddReg

[PortsClass.AddReg]
HKR,,,,%PortsClassName%

[ClassInstall32.NT]
AddReg=PortsClass.NT.AddReg

[PortsClass.NT.AddReg]
HKR,,,,%PortsClassName%
HKR,,Icon,,"-23"
HKR,,Installer32,,"MsPorts.Dll,PortsClassInstaller"

; Drivers
;----------------------------------------------------------
[Manufacturer]
%mfg%=mfg

[mfg]
%ComPort.DeviceDesc%  = ComPort, OXPCIMF\*PNP0501
%ComPort.DeviceDesc%  = ComPort, OX16PCI954\*PNP0501
%ComPort.DeviceDesc%  = ComPort, OX9162\*PNP0501
%ComPort.DeviceDesc%  = ComPort, OXCB950\*PNP0501
%ComPort.DeviceDesc%  = ComPort, OXMF\*PNP0501
%ComPort.DeviceDesc2% = ComPort, OXMFCF\*PNP0501

[ControlFlags]
ExcludeFromSelect = OXPCIMF\*PNP0501
ExcludeFromSelect = OX16PCI954\*PNP0501
ExcludeFromSelect = OX9162\*PNP0501
ExcludeFromSelect = OXCB950\*PNP0501

; ************** install serial ports ***********************
[ComPort]
DriverVer=02/07/2005, 5.1.0
CopyFiles=ComPort.Copy
AddReg=ComPort.AddReg, ComPort.W95.AddReg

[ComPort.NT]
AddReg=ComPort.AddReg, ComPort.NT.AddReg

[ComPort.NT.HW]
AddReg=ComPort.NT.HW.AddReg

[ComPort.NT.HW.AddReg]
HKR,,"UpperFilters", 0x00010000, "serenum"  ;;MULTI_SZ
HKR,,"UpperFilters", 0x00010008, "oxmfuf"   ;;APPEND
HKR,,"95xSpecific",  0x00000001, 01,00,00,00,00,00,c9,16,20,00,01,00,04,64,10,70,08,00,00,00,00,40,00,10
HKR,,"ClockRate",    0x00010001, 1843200
HKR,,"MultiportProperties",0x00010001, 1

[ComPort.AddReg]
HKR,,PortSubClass,1,01

[ComPort.W95.AddReg]
HKR,,DevLoader,,*vcomm
HKR,,Enumerator,,serenum.vxd
HKR,,PortDriver,,oxser.vxd
HKR,,ConfigDialog,,oxserui.dll
HKR,,DCB,3,1c,00,00,00,80,25,00,00,11,33,00,00,00,00,0a,00,0a,00,08,00,00,11,13,00,00,00
HKR,,950Specific,3,00,01,08,10,04,40,40,78,12,14,00,00,00,01,00,00
HKR,,EnumPropPages,,"oxserui.dll,EnumPropPages"

[ComPort.NT.AddReg]
HKR,,EnumPropPages32,,"oxui.dll,SerialPropPageProvider"
HKLM,%ParametersSubKey%, OxfordFlags,   0x00010001,     0


;-------------- Service installation
; Port Driver (function driver for this device)
[ComPort.NT.Services]
AddService = oxser, 0x00000002, oxser_Service_Inst, oxser_EventLog_Inst
AddService = Oxmfuf,,Oxmfuf_Service_Inst
AddService = Serenum,,Serenum_Service_Inst


; -------------- Serial Port Driver install sections
[oxser_Service_Inst]
DisplayName    = %oxser.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 1               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 0               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\oxser.sys
LoadOrderGroup = Extended base

; -------------- Serenum Driver install section
[Serenum_Service_Inst]
DisplayName    = %Serenum.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter

; -------------- Filter Driver install section
[Oxmfuf_Service_Inst]
DisplayName    = %Oxmfuf.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\oxmfuf.sys
LoadOrderGroup = PNP Filter

[oxser_EventLog_Inst]
AddReg = oxser_EventLog_AddReg

[oxser_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\oxser.sys"
HKR,,TypesSupported,0x00010001,7

[ComPort.Copy]
oxser.vxd
oxserui.dll

[ComPort.PosDup]
*PNP0501

[SourceDisksNames]
1=%drvdisk%,,

[SourceDisksFiles]
oxser.vxd=1
oxserui.dll=1

[Strings]
mfg                     = "(Enhanced ports)"
PortsClassName          = "Ports (COM & LPT)"
drvDisk                 = "High-performance ports driver disk"

ComPort.DeviceDesc      = "PCI Communications Port"
ComPort.DeviceDesc2     = "High Speed Communications Port"

oxser.SVCDESC           = "OX16C95x Serial port driver"
Serenum.SVCDESC         = "Serenum Filter Driver"
Oxmfuf.SVCDESC          = "Filter driver for OX16PCI95x ports"
ParametersSubKey        = "SYSTEM\CurrentControlSet\Services\oxser\Parameters"
